/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2023-03-30
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

Through The computer of serial debugging assistant, display the message sent
and received between the MCU and USART1.

The phenomenon of serial assistant can display information from USART1 .

  - USART1(TX:PA9, RX:PA10) and USART2(TX:PA2, RX:PA3) configured as follow:
  - BaudRate    =   115200
  - Word Length =   USART_WordLength_8b
  - Stop Bit    =   USART_StopBits_1
  - Parity      =   USART_Parity_No
  - Hardware flow control disabled (RTS and CTS signals)
  - Receive and transmit enabled

&par Directory contents

  - USART/USART_Interrupt/Source/apm32a0xx_int.c     Interrupt handlers
  - USART/USART_Interrupt/Source/main.c              Main program

&par Hardware and Software environment

  - This example runs on APM32A091 MINI Devices.
