/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2023-03-25
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example describes how to use the 3 ADCs in independent conversions. 
Two of them; ADC1 and ADC3 are transferring continuously converted data using DMA
while ADC2 converted data are stored using End of conversion interrupt.

  - USART1 and USART2 configured as follow:
  - BaudRate = 115200
  - Word Length = USART_WordLength_8b
  - Stop Bit = USART_StopBits_1
  - Parity = USART_Parity_No
  - Hardware flow control disabled (RTS and CTS signals)
  - Receive and transmit enabled

&par Directory contents

  - ADC/ADC_ADC3DMA/src/apm32a10x_int.c     Interrupt handlers
  - ADC/ADC_ADC3DMA/src/main.c              Main program

&par IDE environment

  - MDK-ARM V5.36
  - EWARM V8.50.5.26295
  - ECLIPSE V4.27

&par Hardware and Software environment

  - This example runs on APM32A103_MINI Devices.
