/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2023-03-25
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be usefull and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

The program to show how to use DMA to transfer Data from
memory to TMR1 Capture Compare Register1 to change the Duty Cycle.

  - TMR1 Repetition counter =   6
  - SystemCoreClock         =   72 MHz.
  - TMR1CLK                 =   SystemCoreClock
  - Prescaler               =   71
  - TMR1 counter clock      =   1 MHz
  - TMR1_Period             =   (1000000 / 1000) - 1

each 6 Update Requests, the TMR1 Channel 1 Duty Cycle changes to the next new value:
  - value1 = 800
  - Channel 1 duty cycle = 80%
  - Channel 1N duty cycle = 20%
  - value2 = 400
  - Channel 1 duty cycle = 40%
  - Channel 1N duty cycle = 60%
  - value3 = 200
  - Channel 1 duty cycle = 20%
  - Channel 1N duty cycle = 80%

Display TMR1 waveform by oscilloscope.

&par Hardware Description

  - using TMR8 Channel 1 (PA8) to output PWM
  - using TMR8 Channel 1N (PB13) to output PWM

&par Directory contents

  - TMR/TMR_TMR1DMA/src/apm32a10x_int.c     Interrupt handlers
  - TMR/TMR_TMR1DMA/src/main.c              Main program

&par IDE environment

  - MDK-ARM V5.36
  - EWARM V8.50.5.26295
  - ECLIPSE V4.27

&par Hardware and Software environment

  - This example runs on APM32A103_MINI Devices.
