/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2023-03-25
 *
 * @attention
 *
 *  Copyright (C) 2023 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example provides a description of how to set a communication between two
SPIs in simplex mode and performs a data buffer transfer from SPI1 interrupt for master
 to SPI2 interrupt for slave. If data is sent correctly, the LED2 will light. The LED3 will blinky.

Connect UART1 and SPI pins as follows:
SPI1 NSS     (PA4)   to SPI2 NSS    (PB12)
SPI1 SCK     (PA5)   to SPI2 SCK    (PB13)
SPI1 MOSI   (PA7)  to  SPI2 MOSI (PB14)

&par Directory contents

  - SPI/SPI_Interrupt/src/apm32a10x_int.c     Interrupt handlers
  - SPI/SPI_Interrupt/src/main.c              Main program

&par IDE environment

  - MDK-ARM V5.36
  - EWARM V8.50.5.26295
  - ECLIPSE V4.27

&par Hardware and Software environment

  - This example runs on APM32A103 MINI Devices.
