;/*
; * FreeRTOS Kernel V10.4.3
; * Copyright (C) 2020 Amazon.com, Inc. or its affiliates.  All Rights Reserved.
; *
; * Permission is hereby granted, free of charge, to any person obtaining a copy of
; * this software and associated documentation files (the "Software"), to deal in
; * the Software without restriction, including without limitation the rights to
; * use, copy, modify, merge, publish, distribute, sublicense, and/or sell copies of
; * the Software, and to permit persons to whom the Software is furnished to do so,
; * subject to the following conditions:
; *
; * The above copyright notice and this permission notice shall be included in all
; * copies or substantial portions of the Software.
; *
; * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
; * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS
; * FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR
; * COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER
; * IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN
; * CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
; *
; * https://www.FreeRTOS.org
; * https://github.com/FreeRTOS
; *
; * 1 tab == 4 spaces!
; */

		RSEG ICODE:CODE
		CODE32

	EXTERN vPortPreemptiveTick
	EXTERN vTaskSwitchContext

	PUBLIC vPortYieldProcessor
	PUBLIC vPortStartFirstTask
	PUBLIC vPortPreemptiveTickISR

#include "ISR_Support.h"

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Starting the first task is just a matter of restoring the context that
; was created by pxPortInitialiseStack().
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
vPortStartFirstTask:
	portRESTORE_CONTEXT

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Manual context switch function.  This is the SWI hander.
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
vPortYieldProcessor:
	ADD		LR, LR, #4			; Add 4 to the LR to make the LR appear exactly
								; as if the context was saved during and IRQ
								; handler.

	portSAVE_CONTEXT			; Save the context of the current task...
	LDR R0, =vTaskSwitchContext	; before selecting the next task to execute.
	mov     lr, pc
	BX R0
	portRESTORE_CONTEXT			; Restore the context of the selected task.

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Preemptive context switch function.  This will only ever get used if
; portUSE_PREEMPTION is set to 1 in portmacro.h.
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
vPortPreemptiveTickISR:
	portSAVE_CONTEXT			; Save the context of the current task.

	LDR R0, =vPortPreemptiveTick ; Increment the tick count - this may wake a task.
	MOV lr, pc
	BX R0

	portRESTORE_CONTEXT			; Restore the context of the selected task.


	END

