/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.2
 *
 * @date        2025-05-15
 *
 * @attention
 *
 *  Copyright (C) 2024-2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

The program to show how to configure the TMR1 channel period
and the duty cycle by DMA burst to generate 7 PWM
with 7 different duty cycles (80%, 70%, 60%, 50%, 40%, 30% and 20%).

On the DMA update request, the DMA will do 6 transfers of half words into TMR1
registers (AUTORLD, REPCNT, CC1, CC2, CC3, CC4).
999 will be transferred into AUTORLD
0 will be transferred into REPCNT
800 will be transferred into CC1.
700 will be transferred into CC2.
600 will be transferred into CC3.
500 will be transferred into CC4.

The objective is to generate 7 PWM signal at 1 KHz:
  - SystemCoreClock = 72 MHz.
  - TMR1CLK = SystemCoreClock, Prescaler = 71, TMR1 counter clock = 1 MHz
  - TMR1_Period = (1000000 / 1000) - 1
  - Channel 1 duty cycle = 80%
  - Channel 2 duty cycle = 70%
  - Channel 3 duty cycle = 60%
  - Channel 4 duty cycle = 50%
  - Channel 3N duty cycle = 40%
  - Channel 2N duty cycle = 30%
  - Channel 1N duty cycle = 20%

Display TMR1 waveform by oscilloscope.

&par Hardware Description

  - using TMR1 Channel 1 (PA8) to output PWM
  - using TMR1 Channel 2 (PA9) to output PWM
  - using TMR1 Channel 3 (PA10) to output PWM
  - using TMR1 Channel 4 (PA11) to output PWM
  - using TMR1 Channel 3N (PB15) to output PWM
  - using TMR1 Channel 2N (PB14) to output PWM
  - using TMR1 Channel 1N (PA7) to output PWM

&par Directory contents

  - TMR/TMR_DMABurst/Source/apm32e030_int.c        Interrupt handlers
  - TMR/TMR_DMABurst/Source/main.c                 Main program

&par Hardware and Software environment

  - This example runs on APM32E030 TINY Devices.
