This ARM Cortex-M33 secure/non-secure example project that
shows the setup of the CMSIS-RTOS2 RTX for TrustZone for 
ARMv8-M applications. 

The application uses CMSIS and can be executed on a Fixed
Virtual Platform (FVP) simulation model. The application 
demonstrates three RTOS threads. 


Secure application:
 - Setup code and start non-secure application.

Non-secure application:
 - Calls a secure function from non-secure state.
 - Calls a secure function that call back to a non-secure function.

Output:
Variables used in this application can be viewed in the Debugger
Watch window.