/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.3
 *
 * @date        2025-06-17
 *
 * @attention
 *
 *  Copyright (C) 2022-2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example describes how to configure the TMR3 and TMR4 realize the 32-bit timer.
TMR3 as High 16 bit count value,TMR4 as Low  16 bit count value.
User can view the counter value through serial terminal.

&par Hardware Description

using USART1(TX:PA9、RX:PA10).
  - USART2 configured as follow:
  - BaudRate = 115200
  - Word Length = USART_WordLength_8b
  - Stop Bit = USART_StopBits_1
  - Parity = USART_Parity_No
  - Hardware flow control disabled (RTS and CTS signals)
  - Receive and transmit enabled

&par Directory contents

  - TMR/TMR_32BitCount/Source/apm32e10x_int.c     Interrupt handlers
  - TMR/TMR_32BitCount/Source/main.c              Main program

&par IDE environment

  - MDK-ARM V5.29
  - EWARM V8.50.4.26131
  - ECLIPSE-EMB V4.24.0

&par Hardware and Software environment

  - This example runs on APM32E103 MINI Devices.