/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.1
 *
 * @date        2025-05-31
 *
 * @attention
 *
 *  Copyright (C) 2023-2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */


&par Example Description

The program to show how to configure the TMR2 peripheral to generate
3 different signals with three different delays.

  - SystemCoreClock = 16MHz.
  - TMR2CLK = SystemCoreClock, divider = 16, TMR counter clock = 1 MHz
  - TMR2_Period    = (1000000 / 1000) - 1
  - TMR2 CH1 pulse = 800
  - TMR2 CH1 delay = 800/1MHz = 800us
  - TMR2 CH2 pulse = 600
  - TMR2 CH2 delay = 600/1MHz = 600us
  - TMR2 CH3 pulse = 400
  - TMR2 CH3 delay = 400/1MHz = 400us

&par Hardware Description

using LED2(PB5).
using LED3(PB4).
using TMR2_CH1(PD4).
using TMR2_CH2(PD3).
using TMR2_CH3(PA3).


&par Software Description

TMR2 waveform will be display by oscilloscope.

&par Directory contents

  - TMR2/TMR2_OCActive/Source/apm32f00x_int.c    Interrupt handlers
  - TMR2/TMR2_OCActive/Source/main.c             Main program


&par Hardware and Software environment

  - This example runs on APM32F003 MINI Devices.


&par IDE environment

MDK-ARM V5.36
EWARM V8.50.5.26295
Eclipse V2022-06（4.24.0）
