/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2022-09-29
 *
 * @attention
 *
 *  Copyright (C) 2022 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be usefull and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */


&par Example Description

This example shows how to use TencentOS Tiny for APM32F0xx. There are 4 task
entries in the system. The "start task" will create 3 tasks with the some priority.
Task 1 is used to update the ADC sample values displayed on LCD. Task 2 is used to 
convert the sample value of ADC to the voltage value. Task 3 will print the "hello 
world" string at an interval of one second.

note: This example uses a stripped-down version of TencentOS Tiny. If want to 
use more features of TencentOS Tiny, you need to migrate more contens such as component
and net.

The USART1 is configured as follows:
    - TX:PA9, RX:PA10
    - BaudRate = 115200 baud
    - Word Length = 8 Bits
    - One Stop Bit
    - No parity
    - Hardware flow control disabled (RTS and CTS signals)
    - Receive and transmit enabled

&par Hardware Description
    - RV1 Potentiometer ADC Channel 9 -> PIN PB1
    - Close J12
    - Close J1 and J3

&par Directory contents

  - RTOS/TencentOS_Tiny/Source/apm32f0xx_int.c     Interrupt handlers
  - RTOS/TencentOS_Tiny/Source/main.c              Main program

&par IDE environment

  - MDK-ARM V5.36
  - EWARM V8.50.4.26131

&par Hardware and Software environment

  - This example runs on APM32F072 EVAL Devices.
  - This example runs on TencentOS Tiny(2.5.2).
