/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2022-11-10
 *
 * @attention
 *
 *  Copyright (C) 2022 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example describes how to use FreeRTOS for APM32F107.
For this example, You can see that LED1 is constantly blinking,
and printing information through the serial assistant.

The UART4 is configured as follows:
  - TX:PC10, RX:PC11
  - BaudRate = 115200 baud
  - Word Length = 8 Bits
  - One Stop Bit
  - No parity
  - Hardware flow control disabled (RTS and CTS signals)
  - Receive and transmit enabled

&par Software Description

Please install the following dependencies in the directory where the installation package resides beforehand.
  - Middlewares/FreeRTOS/FreeRTOSv202012.00-LTS.exe   FreeRTOS Software Components

&par Directory contents 

  - RTOS/FreeRTOS/src/apm32f10x_int.c     Interrupt handlers
  - RTOS/FreeRTOS/src/main.c              Main program

&par IDE environment

  - MDK-ARM V5.29
  - EWARM V8.50.5.26295
  
&par Hardware and Software environment

  - This example runs on APM32F107_EVAL Devices.
