/*!
 * @file        readme.txt
 *
 * @brief       This file is routine instruction
 *
 * @version     V1.0.0
 *
 * @date        2025-02-15
 *
 * @attention
 *
 *  Copyright (C) 2025 Geehy Semiconductor
 *
 *  You may not use this file except in compliance with the
 *  GEEHY COPYRIGHT NOTICE (GEEHY SOFTWARE PACKAGE LICENSE).
 *
 *  The program is only for reference, which is distributed in the hope
 *  that it will be useful and instructional for customers to develop
 *  their software. Unless required by applicable law or agreed to in
 *  writing, the program is distributed on an "AS IS" BASIS, WITHOUT
 *  ANY WARRANTY OR CONDITIONS OF ANY KIND, either express or implied.
 *  See the GEEHY SOFTWARE PACKAGE LICENSE for the governing permissions
 *  and limitations under the License.
 */

&par Example Description

This example shows how to:
  - Configure the PLL1 (clocked by HSE) as System clock source
  - Output the System clock(33.6MHz or 20MHz) on MCO pin(PA8)

&par Directory contents

  - RCM/RCM_ClockConfig/Source/apm32f4xx_int.c     Interrupt handlers
  - RCM/RCM_ClockConfig/Source/main.c                     Main program

&par IDE environment

  - MDK-ARM V5.40
  - EWARM V8.50.5.26295
  - Eclipse V2022-06（4.24.0）

&par Hardware and Software environment

  - This example runs on APM32F411 Tiny Devices.
